---
格式版本: 2
标题: "Artec 3D launches Artec Point II metrology-grade laser scanner"
原文链接: "https://www.engineering.com/artec-3d-launches-artec-point-ii-metrology-grade-laser-scanner/"
发布日期: "2026-08-12"
发布时间校准状态: "found"
发布时间需复核: "否"
发布时间来源: "rule:scrape:strict_html_metadata"
发布时间证据: "article:published_time: 2026-08-12T11:54:23+00:00"
发布时间校准原因: "规则确认唯一严格发布时间，来源 scrape:strict_html_metadata"
发布时间校准置信度: "high"
发布时间候选数量: 8
发布时间严格候选数量: 1
发布时间原页读取状态: "source template page reused from URL open"
发布时间未找到原因: ""
发布时间校准时间: "2026-08-13T03:52:03+08:00"
发布时间仲裁状态: "skipped"
发布时间仲裁尝试次数: 0
发布时间仲裁耗时毫秒: 0
发现时间: "2026-08-13T03:49:37+08:00"
入库时间: "2026-08-12T19:52:04.160Z"
来源平台: "Engineering.com 搜索"
搜索渠道: "source_template"
搜索词: "https://www.engineering.com/?s=AI%20Rack"
匹配关键词:
  - "AI Rack"
  - "AI"
相关厂家:
  []
相关专家:
  []
内容类型: "网页"
抓取工具: "Free Fetch + Defuddle"
清洗工具: "Defuddle Markdown + Defuddle/Readability 正文提取"
原始附件:
  []
AI优质: "否"
AI打分: 10
AI分档: "非优质"
AI质检状态: "不通过"
AI打分理由: "资料为Artec 3D激光扫描仪产品发布，与AI Rack/超节点/机柜级AI基础设施完全无关，属于明显无关内容。"
AI质检模型: "ali-deepseek-v4-flash"
AI质检时间: "2026-08-13T03:52:11+08:00"
AI主题相关性: 0
AI来源权威性: 5
AI新颖性: 0
AI技术细节: 0
AI商业部署信号: 0
AI完整性: 5
采集批次: "2026年8月13日1点55分48秒"
采集批次ID: "20260813-015548-033"
去重键: "https://www.engineering.com/artec-3d-launches-artec-point-ii-metrology-grade-laser-scanner"
---

Captures up to 5.8 million points per second with certified 0.02 mm accuracy for industrial inspection and reverse engineering.

Artec 3D has announced [Artec Point II](https://www.artec3d.com/portable-3d-scanners/laser-point), the successor to Artec Point, its target-based handheld laser scanner for industrial metrology. The scanner uses an expanded laser configuration and captures up to 5.8 million points per second, more than double the original model, while maintaining certified 0.02 mm accuracy.

The updated configuration increases the number of laser lines projected in each mode, with 54 lines in ultra-fast scanning mode and 17 parallel lines in hyperfine mode. Operators can switch between three modes using a button: ultra-fast scanning for larger surfaces, hyperfine parallel scanning for detailed features and single-laser mode for deep holes and hard-to-reach areas. The modes support scanning of small components and large assemblies.

Point II’s accuracy and repeatability are verified in an ISO-certified lab. The scanner complies with VDI/VDE 2634 and JJF 1951 standards for metrology applications. It is designed to help quality teams verify parts against specified tolerances.

The palm-sized scanner is lightweight and can be operated one-handed or tilted into confined areas. It has an IP50 rating for dust protection and operates from −10 to 40 °C, supporting use in manufacturing, mold-making, energy and heavy industry environments.

Point II is integrated with [Artec Studio](https://www.artec3d.com/3d-software/artec-studio), Artec 3D’s 3D scanning and processing software. It can also be used with other Artec 3D devices in the same project for applications such as reverse engineering and quality inspection.

Artec Point II is available through Artec 3D’s global network of certified partners and replaces Artec Point in the company’s metrology lineup.

For more information, visit [artec3d.com](https://www.artec3d.com/).
